
FIRMWARE_ROOT=/lib/firmware/raspberrypi/bootloader
FIRMWARE_RELEASE_STATUS="critical"
FIRMWARE_IMAGE_DIR="${FIRMWARE_ROOT}/${FIRMWARE_RELEASE_STATUS}"
FIRMWARE_BACKUP_DIR="/var/lib/raspberrypi/bootloader/backup"
BOOTFS=/boot
USE_FLASHROM=0
EEPROM_CONFIG_HOOK=
